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	Task
	Health
	Safety
	



Hazards Associated with Task

Identify hazards (as applicable) presented by; operations, equipment, vehicles, materials, products, working conditions and environment.

	Raw Risk Rating
	
Controls

Consider the Hierarchy of Controls.
	Residual Risk Rating

	
	
	
	
	Severity
	Probability
	Overall Risk Rating
	
	Severity
	Probability
	  Overall Risk Rating

	Planning and Preparation
	
	
	Misplacement of core line, conduit, boxes or sleeves
	
	
	
	Eng: Provide an accurate and marked deck layout
Adm: Conduct pre-task meetings to review plans and drawings
 PPE: 
	
	
	

	
	
	
	Unclear or conflicting specifications
	
	
	
	Eng: Use updated, approved plans and schematics
Adm: Verify plans with the site supervisor before work begins
PPE: N/A
	
	
	

	Walking on Rebar
	
	x
	Trips, slips, or falls on uneven rebar
	3
	3
	9
	Eng: Use rebar caps and anti-slip coatings where possible
Adm: Enforce strict housekeeping to remove obstructions
 PPE: All required PPE – safety helmet, safety glasses, gloves, hi-visibility, steel-toe boots.
	2
	2
	4

	
	
	x
	Rebar impalement from a fall
	4
	3
	12
	Eng: Install rebar caps or protective barriers over exposed ends
Adm: Train workers on proper rebar navigation techniques
PPE: All required PPE – safety helmet, safety glasses, gloves, hi-visibility, steel-toe boots.
	2
	2
	4

	Measuring and Marking Locations
	
	x
	Slips or trips from tools and materials
	2
	3
	6
	Eng: Provide tool organization solutions
Adm: Enforce housekeeping policies on the deck
PPE: All required PPE – safety helmet, safety glasses, gloves, hi-visibility, steel-toe boots.
	2
	2
	4

	
	x
	
	Prolonged exposure to sun or sever weather
	3
	3
	9
	Eng: Provide shaded work areas or temporary shelters
Adm: Schedule breaks during extreme weather conditions
PPE: Wide-brimmed hats and sunscreen for UV protection; All required PPE – safety helmet, safety glasses, gloves, hi-visibility, steel-toe boots.
	2
	2
	4

	
	x
	
	Strains from repetitive motions (e.g., bending or squatting while measuring)
	2
	3
	6
	Eng: Use ergonomic measuring tools and extendable markers
Adm: Rotate tasks among workers to reduce repetitive strain
PPE: Knee pads or support braces if needed; All required PPE – safety helmet, safety glasses, gloves, hi-visibility, steel-toe boots.
	1
	2
	2

	Using a Drill to Install Boxes and Sleeves
	
	x
	Injuries from drill operation
	2
	3
	6
	Eng: Use drills with safety features, such as auto shut-off
Adm: Train workers on proper drill handling and troubleshooting
PPE: All required PPE – safety helmet, safety glasses, gloves, hi-visibility, steel-toe boots.
	2
	2
	4

	
	
	X
	Contact with drill debris or sparks
	2
	2
	4
	Eng: Use drills with dust and debris collectors
Adm: Limit access to the work area during drilling operations
PPE: 
	2
	1
	2

	Placing and Securing Core Lines
	x
	
	Overreaching or awkward postures
	2
	3
	6
	Eng:
Adm: Train workers to maintain proper body positioning.  Provide Micro-breaks
PPE: All required PPE – safety helmet, safety glasses, gloves, hi-visibility, steel-toe boots.
	1
	2
	2

	
	
	x
	Injuries from securing tools (e.g., pliers, Tie wire)
	2
	3
	6
	Eng: Provide the correct pliers and tie wire
Adm: Train workers on safe tool use and techniques
PPE: All required PPE – safety helmet, safety glasses, gloves, hi-visibility, steel-toe boots.
	2
	1
	2

	Lifting Coreline Reels onto Deck and Setting up on Jack Stands
	x
	
	Strains or sprains from lifting heavy reels
	3
	3
	9
	Eng: Provide mechanical lifting aids, such as hoists or cranes
Adm: Train workers on proper lifting techniques
PPE: Back support belts (if necessary); All required PPE – safety helmet, safety glasses, gloves, hi-visibility, steel-toe boots.
	2
	2
	4

	
	
	x
	Dropping heavy materials
	4
	3
	12
	Eng: Use secure lifting equipment and proper attachment points
Adm: Assign team lifting for heavy or awkward loads
PPE: All required PPE – safety helmet, safety glasses, gloves, hi-visibility, steel toe boots.
	2
	2
	4

	
	
	x
	Incorrect setup of jack stands
	3
	3
	9
	Eng: Use sturdy, level, and load-rated jack stands
Adm: Inspect jack stands for proper condition and placement
PPE: N/A
	2
	2
	4

	Pulling Core Lines
	
	
	Snagging or tangling of core lines
	1
	3
	3
	Eng: Use reels or guides for smooth wire management
Adm: Assign team members to monitor pulling activities
PPE: 
	1
	2
	2

	
	x
	
	Injuries from the pulling force
	2
	3
	6
	Eng: Provide pulling equipment 
Adm: Train workers on safe pulling techniques
PPE: All required PPE – safety helmet, safety glasses, gloves, hi-visibility, steel toe boots.
	2
	1
	2

	Responding to Emergencies
	
	x
	Falls or injuries from deck work
	4
	3
	12
	Eng: Provide accessible first aid stations on each deck level
Adm: Train workers in fall rescue and first aid procedures
PPE: Emergency-specific PPE (e.g., gloves)
	3
	2
	6

	
	
	x
	Transporting injured workers with limited access to the deck
	4
	2
	8
	Eng: Provide deck-level emergency evacuation equipment (e.g., stretcher, pulley system)
Adm: Pre-plan emergency access routes and drills specific to deck work
PPE: High-visibility vests for rescue personnel
	3
	1
	3













Risk Matrix
SeverityProbability

	
	1 - Insignificant
	2 - Minor
	3 - Major
	4 - Severe

	4 - Almost Certain
	Medium 4
	High 8
	Extreme 12
	Extreme 16

	3 - Likely
	Medium 3
	Medium 6
	High 9
	Extreme 12

	2 - Unlikely
	Low 2
	Medium 4
	Medium 6
	High 8

	1 - Rare
	Low 1
	Low 2
	Medium 3
	Medium 4




Probability pertains to the extent of how likely it is for the risk to occur.
The 4 risk rating levels for this component are:
1. Rare – unlikely to happen or has never happened.
2. Unlikely – has the possibility to happen or has happened at least once.
3. Likely – almost sure to happen or has happened multiple times.
4. Almost certain – sure to happen or has happened frequently.

Severity is to determine the level of effects that the hazard could cause.
The 4 risk rating levels for this component are:
1. Insignificant – can cause injuries/illnesses requiring first aid or negligible property damage.
2. Minor – can cause moderate injuries/illnesses requiring medical aid or moderate property damage.
3. Major – can cause irreversible injuries/illnesses requiring long term aid or serious property damage. 
4. Severe – can result in a fatality or irreversible property damage.

Overall Risk Rating
Severity x Probability = Overall Risk Rating
Low - no further action needed; proper control measures are in place.
Medium – proceed with caution and monitor at regular intervals.
High – must be reviewed and reassessed prior to work proceeding.
Extreme – work must be stopped until adequate controls have reduced hazard to an acceptable level.
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	Disclosure: by signing this formal hazard assessment review record I hereby acknowledge that I have participated in the review of this hazard assessment and understand the tasks, hazards, and controls as they written. I agree that I participated in the review of the hazard assessment and understand the engineering, administrative and personal protective equipment that I must use to protect myself from conducting tasks associated with this hazard assessment. 
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