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	Task
	Health
	Safety
	



Hazards Associated with Task

Identify hazards (as applicable) presented by; operations, equipment, vehicles, materials, products, working conditions and environment.

	Raw Risk Rating
	
Controls

Consider the Hierarchy of Controls.
	Residual Risk Rating

	
	
	
	
	Severity
	Probability
	Overall Risk Rating
	
	Severity
	Probability
	  Overall Risk Rating

	Location and Set-Up of Equipment
	
	x
	Physical Hazards Causing Injury to Personnel on the Ground Near Machinery
	2
	2
	4
	Eng: 
Adm: Regular Workplace and Shop Inspections. Housekeeping and ensuring that trip and slip hazards are addressed when encountered on the floor (i.e., laying objects or clutter). New Worker Orientation. 
PPE: Safety Hard Hats, Protective Footwear, Hand Protection/ Gloves (as required).

	2
	1
	2

	
	
	x
	Struck-by hazards by other operators working in the facility or warehouse
	2
	2
	6
	Eng: Physical barriers to keep vehicles and visitors out of the work area. Heavy-gauge safety chain in front of loading dock opening. 
Adm: Eye contact with the operator. Use standard hand signals when noise levels inhibit auditory communication. Powered Mobile Equipment SOP. Using spotters and rear-view mirrors to increase visibility whenever possible. 
PPE: Safety Hard Hats, Hi-visibility stripes, Safety Eyewear, Hearing Protection, Protective Footwear
	2
	2
	4

	
	x
	
	Bodily Contact with Overhead Cage When Mounting the Forklift
	2
	2
	4
	Eng: Firm, level footing on the forklift. Handhold.
 Adm: Pre-trip inspections and safe work procedures. New Worker Orientation. Be careful with footing and use 3-point contact when mounting or dismounting from forklift. 
PPE: Safety Hard Hats, High Visibility Stripes.
	1
	1
	2

	
	
	x
	Body Contact with Pinch Points
	2
	2
	4
	Eng: 
Adm: Avoid moving parts of machinery. Keep fingers, hands, and arms away from backhoe bucket and other pinch points. Powered Mobile Equipment SOP. Lock Out/Tagout Procedures. New Worker Orientation. 
PPE: Safety Hard Hats, High Visibility Stripes, Safety Eyewear, Protective Footwear, Hand Protection/ Gloves (as required).
	2
	1
	2

	Loading and unloading
	
	X
	Machinery – Unguarded Injury
	3
	2
	6
	Eng: Protective guard rails. Audible back-up signal from forklift when operating in reverse. 
Adm: Lifting and Handling Loads SOP, Powered Mobile Equipment SOP, New Worker Orientation. Avoid moving parts of machinery and keep fingers, hands, and arms away from backhoe bucket or pinch points. Working in a buddy-system or using a spotter. 
PPE: Safety Hard Hats, High Visibility Stripes, Safety Eyewear, Hearing Protection, Protective Footwear, Hand Protection (as required).
	2
	2
	4

	
	
	x
	Electrocution - battery power
	3
	2
	6
	Eng: Approved charging cables and charger connector handle
Adm: Powered mobile equipment SOP, new worker orientation, scheduled equipment inspections
PPE: Safety eyewear, protective footwear, hand protection.
	3
	2
	6

	
	
	X
	Excessive Noise Exposure
	3
	2
	6
	Eng:
Adm: Establish forklift working areas. Standard hand signals when noise levels inhibit auditory communication. Working in a buddy system or using a spotter. Work/Rest Cycle. Reduce travel speeds.
 PPE: Wear approved safety ear plugs or muffs when operating forklift or working close to noise source(s). Suitable Footwear, Safety Hard Hats, High Visibility Stripes, Safety Eyewear, Hand Protection (as required).
	3
	1
	3

	
	
	x
	Unsafe Driving Increasing Risk of Collision or Tip Over
	3
	3
	9
	Eng: Audible back-up signal from forklift when operating in reverse. 
Adm: Lifting and Handling Loads SWP, Powered Mobile Equipment SOP. Establish working zones. Personnel on the ground should keep away from the work area. Reduce travel speed. Maintain current operator certification. 
PPE:
	3
	2
	6

	Unloading delivery truck
	
	X
	Blocked Visibility, Leading to Collisions
	3
	3
	9
	Eng: Audible back-up signal from forklift when operating in reverse. 
Adm: Lifting and Handling Loads SWP, Powered Mobile Equipment SOP. Establish working zones. Personnel on the ground should keep away from the work area unless they are required for the task. Reduce travel speed. Working in a buddy system or using a spotter. 
PPE:
	3
	2
	6

	
	
	x
	Lifting Heavy Loads
	3
	2
	6
	Eng: Dolly, Lifting Equipment, Protective Guardrails, Audible backup signal from forklift when operating in reverse. 
Adm: Adequate Amounts of Rest, Stretch and Take Frequent Breaks, SWP Ergonomics, Housekeeping, Pre-Use Inspections, New Worker Orientation, ERP, Two-Worker Carry, Safe Manual Lifting/Carrying Techniques 
PPE: Protective Footwear, Hand Protection (as required)
	2
	2
	4

	
	X
	
	Worker Injury due to Slip/Trip/Fall
	2
	2
	4
	Eng: Grip Mats, Handrails 
Adm: Pre-Use Equipment Inspections and Shop/Warehouse Inspections, Housekeeping, New Worker Orientation. Ensure that the forklift is parked in an authorized area. Be careful with footing and use 3-point contact when mounting or dismounting from forklift. Adequate lighting in shop/warehouse. 
PPE: Protective Footwear, Hand Protection (as required). Head Lamps If Entering poorly lit areas.
	2
	1
	2

	
	
	X
	Falling Objects Causing Injury to Workers
	3
	3
	9
	Eng: Overhead guards on forklifts to protect operators, 
Adm: Using headlights when lighting is dim or when operating at night. Regularly check overhead guard for broken welds, missing bolts, or other damage. Loading and Transporting Equipment Safe Work Procedure. Establishing no-work zones to limit traffic in area. 
PPE: Safety Hard Hats, High Visibility Stripes, Safety Eyewear, Hearing Protection, Protective Footwear, Hand Protection (as required).
	2
	2
	4

	Preventative Maintenance of Forklift – completed by authorized organization
	
	X
	Changing Hoses Causing Splash/Spill - Chemical burn / Absorption
	2
	3
	6
	Eng: 
Adm: Preventive Maintenance Program, Manufacturer’s Specifications, Out of Service Tag/Sign, Spill Response, Training, New Worker Orientation. Ensure that the forklift is parked in an authorized area. 
PPE: Fire-Resistant Clothing with High Visibility Stripes, Safety Eyewear, Protective Footwear, Hand Protection/Gloves (as required).
	1
	2
	2

	
	
	X
	Changing Oil Causing Splash/Spill - Chemical burn / Absorption
	2
	3
	6
	Eng: 
Adm: Preventive Maintenance Program, Manufacturer’s Specifications, Out of Service Tag/Sign, Spill Response, Training, New Worker Orientation. Ensure that the forklift is parked in an authorized area. 
PPE: Fire -Resistant Clothing with High Visibility Stripes, Safety Eyewear, Protective Footwear, Hand Protection/Gloves (as required).
	2
	1
	2










Risk Matrix
SeverityProbability

	
	1 - Insignificant
	2 - Minor
	3 - Major
	4 - Severe

	4 - Almost Certain
	Medium 4
	High 8
	Extreme 12
	Extreme 16

	3 - Likely
	Medium 3
	Medium 6
	High 9
	Extreme 12

	2 - Unlikely
	Low 2
	Medium 4
	Medium 6
	High 8

	1 - Rare
	Low 1
	Low 2
	Medium 3
	Medium 4




Probability pertains to the extent of how likely it is for the risk to occur.
The 4 risk rating levels for this component are:
1. Rare – unlikely to happen or has never happened.
2. Unlikely – has the possibility to happen or has happened at least once.
3. Likely – almost sure to happen or has happened multiple times.
4. Almost certain – sure to happen or has happened frequently.

Severity is to determine the level of effects that the hazard could cause.
The 4 risk rating levels for this component are:
1. Insignificant – can cause injuries/illnesses requiring first aid or negligible property damage.
2. Minor – can cause moderate injuries/illnesses requiring medical aid or moderate property damage.
3. Major – can cause irreversible injuries/illnesses requiring long term aid or serious property damage. 
4. Severe – can result in a fatality or irreversible property damage.

Overall Risk Rating
Severity x Probability = Overall Risk Rating
Low - no further action needed; proper control measures are in place.
Medium – proceed with caution and monitor at regular intervals.
High – must be reviewed and reassessed prior to work proceeding.
Extreme – work must be stopped until adequate controls have reduced hazard to an acceptable level.
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	Disclosure: by signing this formal hazard assessment review record I hereby acknowledge that I have participated in the review of this hazard assessment and understand the tasks, hazards, and controls as they written. I agree that I participated in the review of the hazard assessment and understand the engineering, administrative and personal protective equipment that I must use to protect myself from conducting tasks associated with this hazard assessment. 
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