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	Task
	Health
	Safety
	



Hazards Associated with Task

Identify hazards (as applicable) presented by; operations, equipment, vehicles, materials, products, working conditions and environment.

	Raw Risk Rating
	
Controls

Consider the Hierarchy of Controls.
	Residual Risk Rating

	
	
	
	
	Severity
	Probability
	Overall Risk Rating
	
	Severity
	Probability
	  Overall Risk Rating

	Use of Powered Hand Tools
	
	X
	Cable Tangling/Kinking
	1
	3
	3
	Eng: 
Adm: Signage, SWP, Safety Program, Housekeeping, Pre-Use Inspections, New Worker Orientation, Manufacturer’s Instructions 
PPE: Hand Protection, safety eyewear, hard hat, steel-toed boots, hearing protection (as required)
	1
	2
	2

	
	
	X
	Worker injury due to Electric Shock
	2
	2
	4
	Eng: 
Adm: Signage, SWP, Safety Program, Housekeeping, Pre-Use Inspections, New Worker Orientation, ERP 
PPE:  Hand Protection, safety eyewear, hard hat, steel-toed boots, hearing protection (as required)
	2
	1
	2

	
	
	X
	Worker Injury Due to Broken Tools
	3
	2
	6
	Eng: 
Adm: Ergonomics Training, Signage, SWP, Safety Program, Housekeeping, Pre-Use Inspections, New Worker Orientation, ERP
 PPE:  Hand Protection, safety eyewear, hard hat, steel-toed boots, hearing protection (as required)
	3
	1
	3

	
	
	X
	Heavy Manual Lifting Causing Injury
	2
	2
	4
	Eng: Dolly / Mechanical assist device. 
Adm: Ergonomics Training, Signage, SWP, Safety Program, Housekeeping, Pre-Use Inspections, New Worker Orientation, ERP 
PPE.   Safety Hard Hats, High Visibility Stripes, Safety Eyewear, Hand Protection, Steel-Toed Boots, hearing protection (as required)
	2
	1
	2

	
	
	X
	Force / Pressure Causing Injury
	3
	2
	6
	Eng: 
Adm: Ergonomics Training Program, SWP Ergonomics, Avoid Prolonged or Excessive Grasping of Tools, Work / Rest Cycle PPE:   Safety Hard Hats, High Visibility Stripes, Safety Eyewear, Hand Protection, Steel-Toed Boots, hearing protection (as required)
	2
	2
	4

	
	X
	
	Excessive Vibration
	3
	2
	6
	Eng: 
Adm: Ergonomics Training, SWP Ergonomics, Avoid Prolonged or Excessive Grasping of Tools, Work / Rest Cycle 
PPE:   Safety Hard Hats, High Visibility Stripes, Safety Eyewear, Hand Protection, Steel-Toed Boots, hearing protection (as required)
	2
	2
	4

	
	
	X
	Worker Injury Due to Slip/Trip/Fall
	2
	2
	4
	Eng: 
Adm: Aware of Ground Conditions, Signage, SWP, Housekeeping, Pre-Use Inspections, New Worker Orientation. PPE:  Safety Hard Hats, High Visibility Stripes, Safety Eyewear, Hand Protection, Steel-Toed Boots, hearing protection (as required)
	2
	1
	2

	
	X
	
	Awkward Posture / Body Position or Hold
	3
	2
	6
	Eng: Machine Guards 
Adm: Training, Signage, SWP, Housekeeping, Pre-Use Inspections, New Worker Orientation, ERP, Proper Tool Selection, Adequate Lighting 
PPE:   Safety Hard Hats, High Visibility Stripes, Safety Eyewear, Hand Protection, Steel-Toed Boots, hearing protection (as required)
	3
	1
	3

	
	
	X
	Use of Wrong Tools for the Task Causing Injury
	3
	2
	6
	Eng: 
Adm: Worker Training and Competency Program, On-the-Job Training, Pre-Use Inspections, New Worker Orientation, ERP PPE:  Safety Hard Hats, High Visibility Stripes, Safety Eyewear, Hand Protection, Steel-Toed Boots, hearing protection (as required)
	2
	2
	4

	
	
	X
	Congested Work Areas (Tight Spaces, Other Workers, etc.
	2
	2
	4
	Eng: 
Adm: Signage, SWP, Housekeeping, Pre-Use Inspections, New Worker Orientation, Establishment of Exclusion Zones 
PPE:  Safety Hard Hats, High Visibility Stripes, Safety Eyewear, Hand Protection, Steel-Toed Boots, hearing protection (as required)
	2
	1
	2

	
	X
	
	Flying Debris
	3
	2
	6
	Eng: Guards, Vacuum Dust Suppression, Ventilation 
Adm: Signage, SWP Tool Operation, Housekeeping, Pre-Use Inspections, New Worker Orientation, Establishment of Exclusion Zones 
PPE:  Safety Hard Hats, High Visibility Stripes, Safety Eyewear, Hand Protection, Steel-Toed Boots, hearing protection (as required)
	3
	1
	3

	
	
	x
	Blade/Bit Failure Causing Injury
	3
	3
	9
	Eng: Machine Guards 
Adm: Pre-Use Inspection, Preventative Maintenance Program, Worker Training / Competency Program, SWP Tool Operation PPE:  Safety Hard Hats, High Visibility Stripes, Safety Eyewear, Hand Protection, Steel-Toed Boots, hearing protection (as required)
	2
	2
	4

	
	
	X
	Body Part Contracting Pinch Point
	3
	2
	6
	Eng: Machine Guards 
Adm: SWP Ergonomics, SWP Tool Operation, Worker Training / Competency Program, Signage, Housekeeping, Pre-Use Inspections, New Worker Orientation, Adequate Lighting 
PPE:  Safety Hard Hats, High Visibility Stripes, Safety Eyewear, Hand Protection, Steel-Toed Boots, hearing protection (as required)
	2
	1
	2

	
	X
	
	Dust (Inhalation)
	3
	2
	6
	Eng: Vacuum Dust Suppression, Ventilation 
Adm: Fit testing for masks, Worker Training / Competency Program, SWP Tool Operation, Signage, Communication Procedures 
PPE: N95 Mask, Head Protection, Safety Hard Hats, High Visibility Stripes, Safety Eyewear, Hand Protection, Steel-Toed Boots, hearing protection (as required)
	2
	2
	4

	
	
	X
	Dust (Explosive Atmosphere)
	3
	3
	9
	Eng: Vacuum Dust Suppression 
Adm: No smoking policy, Worker Training / Competency Program, SWP Tool Operation, Signage, Communication Procedures 
PPE: N95 Mask, Head Protection, Safety Hard Hats, High Visibility Stripes, Safety Eyewear, Hand Protection, Steel-Toed Boots, hearing protection (as required)
	2
	2
	4

	
	X
	
	Excessive Noise
	3
	2
	6
	Eng: 
Adm: Regular Maintenance on Tools and Equipment, Work Rotation, Establishment of Exclusion Zones
PPE:  Head Protection, Safety Hard Hats, High Visibility Stripes, Safety Eyewear, Hand Protection, Steel -Toed Boots, hearing protection (ear plugs or earmuffs)
	2
	2
	4

	
	
	X
	Falling Material Causing Worker Injury
	3
	2
	6
	Eng: Safety Nets (where possible), Clamps 
Adm: Training, Cargo Securement Requirements, Signage, SWP, Housekeeping, Pre-Use Inspections, New Worker Orientation, ERP, Safe Manual Lifting / Carrying Techniques, Temporary Blockades to Prevent Worker Crossing 
PPE:  Safety Hard Hats, High Visibility Stripes, Safety Eyewear, Hand Protection, Steel-Toed Boots, hearing protection (as required)
	2
	2
	4












Risk Matrix
SeverityProbability

	
	1 - Insignificant
	2 - Minor
	3 - Major
	4 - Severe

	4 - Almost Certain
	Medium 4
	High 8
	Extreme 12
	Extreme 16

	3 - Likely
	Medium 3
	Medium 6
	High 9
	Extreme 12

	2 - Unlikely
	Low 2
	Medium 4
	Medium 6
	High 8

	1 - Rare
	Low 1
	Low 2
	Medium 3
	Medium 4




Probability pertains to the extent of how likely it is for the risk to occur.
The 4 risk rating levels for this component are:
1. Rare – unlikely to happen or has never happened.
2. Unlikely – has the possibility to happen or has happened at least once.
3. Likely – almost sure to happen or has happened multiple times.
4. Almost certain – sure to happen or has happened frequently.

Severity is to determine the level of effects that the hazard could cause.
The 4 risk rating levels for this component are:
1. Insignificant – can cause injuries/illnesses requiring first aid or negligible property damage.
2. Minor – can cause moderate injuries/illnesses requiring medical aid or moderate property damage.
3. Major – can cause irreversible injuries/illnesses requiring long term aid or serious property damage. 
4. Severe – can result in a fatality or irreversible property damage.

Overall Risk Rating
Severity x Probability = Overall Risk Rating
Low - no further action needed; proper control measures are in place.
Medium – proceed with caution and monitor at regular intervals.
High – must be reviewed and reassessed prior to work proceeding.
Extreme – work must be stopped until adequate controls have reduced hazard to an acceptable level.
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	Disclosure: by signing this formal hazard assessment review record I hereby acknowledge that I have participated in the review of this hazard assessment and understand the tasks, hazards, and controls as they written. I agree that I participated in the review of the hazard assessment and understand the engineering, administrative and personal protective equipment that I must use to protect myself from conducting tasks associated with this hazard assessment. 
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